ITEM #: DUMP SINK  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: SC18W  
Pertinent Data: ---  
Utilities Req’d: 1/2” HW, 1/2” CW; 1-1/2” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide a 10” x 14” x 9-1/2” sink bowl with faucet.  
3. Provide a 5” diameter waste chute with 5/8” raised rim.  
4. Equip unit with stainless steel outer and inner door panels (SCDR18) with right hinge and dual magnetic catch.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.