ITEM # : DUMP SINK   
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSF12PS-SR  
Pertinent Data: With Glass Rinser  
Utilities Req’d: 1/2” HW, 1/2" CW; 1-1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide cutting board, 1” thick white PVC, with drip groove.  
3. Provide 4-3/8" diameter heavy gauge stainless steel rack, NSF-listed stainless steel rinser.  
4. Provide 5.5” OD Stainless steel tool well with removable basket, and chrome plated fine-stream faucet.  
5. Sink bowl to be stainless steel, all horizontal and vertical edges 1-1/2" radius with balled corners and furnished with 1-1/2" drain socket.  
6. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.  
7. Provide 6" backsplash.  
8. Provide Perlick Flex Mount Leg Relocation Kit, Includes: (2) Rails, (2) Bolts, and (2) Tightening Knobs, For Perlick Prep Sinks.  
9. Provide 934GN-LF Front Loading Faucet, wall/splash mount, lead free, gooseneck spout, faucet valves includes: built-in check valves to prevent back flow or across flow, (2) 3/8" O.D. x 3/8" O.D. x 18", with braided stainless steel supply lines included.  
10. Provide 7055-52 Perforated Wet Waste Pan, 2.7-quart capacity, clear plastic, for 12"W & 14"W blender stations (6-3/8" x 10-3/8" x 4" deep).  
11. Provide GR-IK Water Pressure Regulator Parts Bag for glass rinser.  
12. Provide shop drawings for approval prior to fabrication.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.