ITEM #: ELECTRONIC READOUT  
Quantity: One (1)  
Manufacturer: Cardinal  
Model No.: 205  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 5.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a push button tare.  
4. Provide Gross, tare, net conversion.  
5. Provide selectable key lockout.  
6. Provide auto shutoff and sleep modes.  
7. Provide four input lines.  
8. Coordinate installation with and connect to Item #, Floor Scale.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.