ITEM #: ESPRESSO GRINDER  
Quantity: One (1)  
Manufacturer: La Marzocco  
Model No.: Swift  
Pertinent Data: ----  
Utilities Req’d: 120V/1PH 12.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide the Swift grinder’s engineering and design to guarantee level and consistent coffee beds.  
4. Equip unit with flat ceramic burrs which ensure minimal heat buildup during the grinding process enabling the unit to be the ideal grinder for high-volume café locations aiming to improve consistency.   
5. Unit shall feature dual hopper design, the unit allows for a single grinder to serve two different coffees.  
6. The unit shall offer highly accurate volumetric dosing and tamping, the Swift repeatedly doses to within a fraction of a gram.  
7. Provide a step-less micro grind adjustment which provides the barista with the highest level of control, while also minimizing waste.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.