ITEM #: ESPRESSO MACHINE  
Quantity: One (1)  
Manufacturer: Franke  
Model No.: A300 FM EC  
Pertinent Data: Automatic  
Utilities Req’d: 208V/1PH; 10.0A; 3/8" CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide double bean hoppers of 2.5 pounds capacity each.  
4. Provide precision grinder with durable ceramic grinding disks.  
5. Provide one touch grind, tamp and brew.  
6. Provide FoamMaster for milk foam.  
7. Provide interactive 8” touch screen guides.  
8. Provide one powder dosing system.  
9. Provide automatic cleaning and rinsing program.  
10. Provide and coordinate installation of a Water Filtration System.  
11. Provide machine install, start-up and calibration of equipment by Franke authorized service partner.  
12. Provide Installation Kit, which includes (1) jar cleaning tablet, water hose and BSP connector, water hardness test strip, piston o-ring change instructions, espresso shot guideline stickers, MSDS sheets for cleaning tablets only, technical support sticker and milk cleaner.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.