ITEM # : ESPRESSO MACHINE  
Quantity: One (1)   
Manufacturer: Schaerer  
Model No.: Coffee Art Plus  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 30.0A; 3/8" CW; 1-1/2" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 30 programmable selections.  
4. Provide grind, tamp and brew settings are programmable for each espresso selection.  
5. Program shall include temperature and texture settings (cappuccino & latte) that are pro-grammable for each steaming selection.  
6. Provide steam wand with finesteam air injection and auto shut-off.  
7. Provide revolutionary PEEK steam wand material to lower the wand’s surface tempera-ture.   
8. Unit shall be equipped with push-button operation.  
9. Equip unit with dual bean hoppers with dedicated grinders for multiple bean types.  
10. Unit shall steam 32oz of milk in 1 minute, and have the ability to serve 70-80 cappucci-nos/lattes per hour (16oz).  
11. Provide 2-step installation, start-up, and calibration.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.