ITEM #: EYE WASH STATION  
Quantity: One (1)  
Manufacturer: Bradley  
Model No.: S19-220BPT  
Pertinent Data: ---  
Utilities Req’d: 1/2" CW, 1/2" HW; 1-1/4" DW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with S19-2000 Navigator EFXB emergency thermostatic mixing valve.  
4. Provide unit with stainless-steel bowl.  
5. Provide large push handle for high visibility in emergency situations is operated by hand.  
6. Provide heavy-gauge sand cast aluminum protected with BradTect safety yellow coating. Includes three clearance holes for mounting bracket onto wall.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.