ITEM #: FILLER FAUCET  
Quantity: One (1)  
Manufacturer: Fisher  
Model No.: 4231  
Pertinent Data: ---  
Utilities Req’d: 1/2” CW, 1/2” HW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with 11” control swing spout and 13” double jointed assembly.  
3. Provide pot filler spout with shutoff valve.  
4. Provide unit with wrist-blade handles.  
5. Coordinate installation on Item #\_\_  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.