ITEM #: FILLER FAUCET  
Quantity: One (1)  
Manufacturer: Fisher  
Model No.: 5440  
Pertinent Data: ---  
Utilities Req’d: 3/4” CW, 3/4” HW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with 72” hose.  
3. Provide pot filler spout with shutoff valve, nonmarring on a 360-degree swivel elbow.  
4. Provide unit with inline dual check valve, and back flow preventors.  
5. Provide unit with wrist-blade handles.  
6. Provide unit with pipe hook.  
7. Coordinate installation on Item #, Preparation Table with Bain Marie.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.