ITEM # : FILLER PIECE   
Quantity: One (1)  
Manufacturer: Perlick   
Model No.: Custom Design  
Pertinent Data: ---   
Utilities Req’d: 1" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have drainboard top.  
3. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.  
4. Unit shall be constructed of embossed stainless steel drainboard.  
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.