ITEM #: FISH FILE REFRIGERATOR  
Quantity: One (1)  
Manufacturer: Victory   
Model No.: RS-1D-S1-HC-FF  
Pertinent Data: Single Section, Self-Contained  
Utilities Req’d: 120V/1PH; 6.5A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide stainless steel exterior, and interior.  
3. Provide stay-open drawer feature for easy product loading.  
4. Equip unit with one-piece, snap-in magnetic drawer gaskets.  
5. Unit shall have stainless steel pans that drain independently into main drain line.  
6. Provide low profile horizontal drawer handles.  
7. Equip unit with hinged front shroud makes condenser cleaning easier.  
8. Provide 6” high adjustable stainless steel legs.  
9. Unit shall have heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.