ITEM #: FISH PREPARATION TABLE WITH SINK  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans Drawing #FS  
Utilities Req’d: (2) 120V/1PH; 20.0A; (Convenience Outlet)  
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #1A, #2B, #4C, #5A, and #15.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide flanged feet on front feet only to secure to floor.  
5. Unit shall be equipped 16-gauge 304 stainless steel under shelf with 2” turn-up at the rear.  
6. Coordinate installation of Item #, PreRinse Unit with Faucet.  
7. Provide cutout in table top with support tabs and pins for Item #, Recessed Cutting Board.  
8. Provide cutout in table for Item # Fish Sink with Perforated Bottom.  
9. Provide a fully enclosed back splash on left side of the table.  
10. Coordinate installation with Item #, Double Wall Shelf, and Item #, Knife Sanitizer.  
11. Provide space under table for Item #, Trash Receptacle.  
12. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.  
13. Provide shop drawings for approval prior to fabrication.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.