ITEM #: FLOOR SCALE  
Quantity: One (1)  
Manufacturer: Cardinal  
Model No.: FHN544/PTN44  
Pertinent Data: Recessed  
Utilities Req’d: 120V/1PH; 15.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide diamond plate platform material.  
4. Equip unit with 4 sealed electronic strain gage load cells as weighing elements.  
5. Provide calibration controls.  
6. Provide platform restraint with self-checking load cells.  
7. Provide adjustable leveling feet mounted to each load cell.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.