ITEM #: FOOD TRANSPORT CART  
Quantity: One (1)  
Manufacturer: FWE  
Model No.: TS-1826-18  
Pertinent Data: Stainless Steel Exterior  
Utilities Req’d: 120V/1PH; 11.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with standard single door.  
3. Provide a patented built-in AHumi-Temp@ system which shall include an Incoloy nickel-chromium alloy heating element and Hi-Temp, self-lubricated, impedance protected fan-cooled blower motor.  
4. Provide unit with removable, oversized humidity reservoir.  
5. Provide unit with all welded construction.  
5. Provide unit with recessed eye level controls.   
6. Provide unit with heavy duty cord and plug, coordinate NEMA configurations with electrical contractor.   
7. Provide four (4) heavy duty all swivel casters, two (2) with brakes.  
8. Provide unit with a digital thermometer.  
9. Provide a 2000 watt element.  
10. Provide a heat retention battery.  
11. Provide a key locking door latch.  
12. Provide unit with a full extension bumper.  
13. Provide unit with extra tray slides.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.