ITEM #: FOOD WASTE COLLECTOR  
Quantity: One (1)  
Manufacturer: InSinkErator  
Model No.: PRP  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH, 3.2A; 1/2“ HW, 1/2” CW, 2” DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation of unit into Item #, Pot Sink as shown on drawing.  
3. Provide with a Control Center with a remote mounting bracket.  
4. Provide with solenoid valve, syphon breaker, and flow control valve.  
5. Provide a remote StartStop.  
6. Provide a cover.  
7. Provide an additional Scrap Basket.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.