ITEM #: FOOD WASTE COLLECTOR  
Quantity: One (1)  
Manufacturer: InSinkErator  
Model No.: PRS  
Pertinent Data:   
Utilities Req’d: 208V/3PH, 3.2A; 1/2” HW, 1/2” CW, 2” DW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation of unit into Item #, Soiled Dish Table as shown on drawing.  
3. Provide with a Control Center with a remote mounting bracket.  
4. Provide with solenoid valve, syphon breaker, and flow control valve.  
5. Provide a remote StartStop.  
6. Provide a cover.  
7. Provide an easy access ball valve allows operators to quickly reposition water plume.  
8. Provide an additional Scrap Basket.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.