ITEM #: FOUR BURNER RANGE  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: IHR4C  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 6.0A; 3/4” Gas @ 175,000 BTUs; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a convection oven with a high-performance stainless steel unique burner at 35,000 Btu/hour.  
4. Provide wavy grates.  
5. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
6. Provide cast iron design features flame shaping center tube for more efficient heat transfer.  
7. Provide porcelainized interior sides rear and deck on oven.  
8. Provide a single deck high shelf SHS36.  
9. Provide a 3/4” LP Gas shut off valve.  
10. Provide 48” flex, quick disconnect gas hose with restraining device and LP Gas pressure regulator.  
11. Provide PosiSet.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.