ITEM #: FRENCH TOP RANGE  
Quantity: One (1)  
Manufacturer: Jade Range  
Model No.: JTRH-2FHT-36C  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 4.0A; 3/4” Gas @ 90,000 BTU’s   
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a convection oven with a high-performance stainless steel unique burner at 30,000 BTU’s.  
4. Provide two (2) highly polished cast iron French tops.  
5. Equip unit with cast iron rings and lids easily removable to deliver direct flame.  
6. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
7. Provide cast iron design features flame shaping center tube for more efficient heat transfer.  
8. Equip unit with a stainless steel 6” plate shelf.  
9. Provide 14-gauge stainless steel interior sides rear and deck on oven.  
10. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
11. Provide PosiSet.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.