ITEM #: FROST TOP  
Quantity: One (1)  
Manufacturer: Wells  
Model No.: FT-3  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 5.6A; 1” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide the top of die stamped stainless steel construction with a 1” drain.  
4. Provide remote On/off switch with 8 ft. cord & plug for ease of installation and operation.  
5. Provide a five-year compressor Warranty.  
6. Coordinate installation into Item #, Service Counter with Trayslide.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.