ITEM #: FRYER  
Quantity: One (1)  
Manufacturer: Jade  
Model No.: JTFF-40-18  
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 122,000 BTU’s; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 3/4” rear gas connection, cap and cover front gas manifold on both left and right side.  
4. Provide stainless steel tank.  
5. Equip unit with stainless steel front, sides and top.  
6. Unit shall be equipped with 32mm quick drain port.  
7. Provide heavy-gauge stainless steel fryer baskets.  
8. Equip unit with four (4) 6” casters front two with brakes.  
9. Provide a stainless steel 6” plate shelf.  
10. Unit shall be provided with a stainless steel door.  
11. Equip unit with a 12” stainless steel Short Riser.  
12. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
13. Provide PosiSet.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.