ITEM #: GLASS FILLER FAUCET  
Quantity: One (1)  
Manufacturer: Fisher  
Model No.: 1117WB   
Pertinent Data: ---  
Utilities Req’d: 1/2” CW, 1/2” HW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation onto deck of Item #, Beverage Counter With Sink.  
3. Provide with wall bracket.  
4. Provide a 12” swing spout.  
5. Provide backflow preventer.  
6. Provide unit with wrist-blade handles.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.