ITEM #: GLASS RINSER  
Quantity: One (1)  
Manufacturer: Micro Matic  
Model No.: MM5821   
Pertinent Data: ---  
Utilities Req’d: 1/2” CW, 1/2” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide robust 10-gauge stainless steel for durable long-lasting performance.  
4. Equip unit with an inline water regulator set at 1.03 bar from the street water supply.  
5. Unit shall install a shutoff on the rinser water supply.  
6. Coordinate installation into Item #, Beverage Counter.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.