ITEM #: GLASSWASHER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: PKHT24  
Pertinent Data: Single Tank  
Utilities Req’d: 208V/1PH; 33.0A; 1/2” HW; 1” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be provided with built-in 70 degree rise booster heater.  
3. Unit shall be provided with SafetyTemp feature ensures proper temperatures in the final rinse.  
4. Unit shall be provided with built-in detergent and rinse aid pumps.  
5. Provide shop drawings for approval prior to installation.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.