ITEM #: GRIDDLE  
Quantity: One (1)  
Manufacturer: Jade Range  
Model No.: JTRH-36GT-36C  
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 120,000 BTU’s, 5” WC

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Set in place in location as shown on drawings.  
2. Provide 1” thick polished steel plate.  
3. Provide thermostatic controls.  
4. Equip unit with stainless steel grease trough.  
5. Unit shall be equipped with a stainless steel tray bed, deflectors, tray guides, drip tray and grease can.  
6. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
7. Provide cast iron design features flame shaping center tube for more efficient heat transfer.  
8. Equip unit with a stainless steel 6” plate shelf.  
9. Provide a convection oven with a high-performance stainless steel unique burner at 30,000 BTU’s.  
10. Provide 14-gauge stainless steel interior sides rear and deck on oven.  
11. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
12. Provide PosiSet.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.