ITEM #: HAND SINK  
Quantity: One (1)  
Manufacturer: Advance Tabco  
Model No.: 7-PS-68  
Pertinent Data: With Vendor Supplied Soap And Towel Dispenser  
Utilities Req’d: 1/2” HW, 1/2” CW; 1-1/2” DW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with gooseneck faucet.  
3. Provide unit with P-trap and tail piece.  
4. Provide battery-operated faucet. (K-175 swing spout faucet).  
5. Provide 6 Volt battery to operate electronic sensor.  
6. Provide 12” welded side splash on each side (7-PS-11).  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.