ITEM #: HEATED BANQUET CART  
Quantity: Five (5)  
Manufacturer: Carter Hoffmann  
Model No.: BR150  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 15.3A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide completely welded double wall cabinet construction with outer cabinet formed and welded to base.  
4. Provide type 300 series stainless steel; 20-gauge polished exterior and 24-gauge interior.  
5. Provide four (4) 6” diameter heavy-duty, non-marking, balloon casters, all with brakes.  
6. Provide wrap around bumper of non-marking gray vinyl bumper set in heavy-duty 3/16” thick extruded aluminum frame with reinforced corner cutouts.  
7. Provide two doors with 16-gauge stainless steel full length 1” tubular hinges.  
8. Provide two (2) 1” diameter 18-gauge stainless steel tubular handles bolted to cabinet with 12-gauge backup plates.  
9. Provide 12-gauge stainless steel top mounted transport latches with padlock provision.  
10. Provide three (3) welded duplex nickel-plated removable wire shelves.  
11. Provide dial type with remote sensing bulb and sensing bulb protector, mounted to center mullion.  
12. Provide bottom mounted heater.  
13. Provide 150 covered plate capacity.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.