ITEM #: HEATED CABINET  
Quantity: One (1)  
Manufacturer: CresCor  
Model No.: 1000-HH-SS-2DE  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 15.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide latch chrome plated zinc with composite handle, magnetic type; mounted inboard.  
4. Provide four (4) 5” heavy-duty, non-marking casters front two (2) with brakes.  
5. Unit shall be constructed of Type 304 stainless steel; 22-gauge polished exterior; 18-gauge interior.  
6. Provide solid dutch doors formed 20-gauge stainless steel with perimeter type silicon gaskets and adjustable vents.  
7. Provide pane slides shall be wire rack with .250 dia. wire vertically and .208 dia. wire horizontally. Nickel chrome plated steel spaced on 2-3/4” centers.   
8. Provide Electronic temperature control with digital temperature display. Display accurate to ±2˚F.   
9. Provide an 1800 Watt heating system maintains the right temperature to properly hold products. Heats up to 200°F. (93°C.).   
10. Provide with heavy-duty cord and plug. Coordinate NEMA configuration with Electrical Contractor.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.