ITEM #: HEATED CABINET  
Quantity: Two (2)  
Manufacturer: FWE  
Model No.: HLC-7  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 4.3A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heliarc welded, single unit construction of stainless steel.  
4. Provide heavy-duty stainless steel, side-mounted lift handles.  
5. Provide flush mounted, double pan, stainless steel door.  
6. Provide high temperature door gasket.  
7. Provide flush in-door stainless steel paddle latch.  
8. Provide four (4) heavy duty, non-marking, polyurethane swivel casters, two (2) with brakes.  
9. Provide a radiant heat system shall include an Incoloy nickel-chromium alloy heating element.  
10. Provide a removable stainless steel humidifier pan.  
11. The unit controls shall be up-front, recessed and shall include a full range thermostat adjustable to actual temperature.  
12. Coordinate installation under Item #, Work Counter with Sink.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.