ITEM #: HEATED CABINET  
Quantity: One (1)  
Manufacturer: FWE  
Model No.: PH-1826-18  
Pertinent Data: Stainless Steel Exterior  
Utilities Req’d: 120V/1PH, 13.8A Each  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide manual controls with digital thermometer.  
3. Provide unit with magnetic latch.  
4. Provide unit with full extension bumper.  
5. Provide unit with floor lock.   
6. Provide unit with heavy duty cord and plug, coordinate NEMA configurations with electrical contractor.   
7. Provide four (4) heavy duty all swivel casters, two (2) with brakes.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.