ITEM #: HEATED DECK  
Quantity: Two (2)  
Manufacturer: Hatco  
Model No.: GRSB60F  
Pertinent Data: Built-In  
Utilities Req’d: 120V/1PH; 7.9A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation into Item #, Work Counter.  
4. Provide a thermal break for the solid surface counter top.  
5. Provide flush mount unit with electronic control box with lighted power switch attached to stainless steel apron bracket on Item #, Work Counter.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.