ITEM #: HEATED DRAWERS  
Quantity: One (1)  
Manufacturer: Hatco  
Model No.: HDW3B  
Pertinent Data: 3 Drawers  
Utilities Req’d: 120V/1PH; 11.3A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation into Item #, Room Service Setup Counter With Sink.  
4. Provide each drawer with a recessed individual thermostatic control, temperature monitor, and On/Off switch.  
5. Equip unit with heavy-duty drawer slides with nylon rollers.  
6. Unit shall be equipped with adjustable sliding vents on each drawer.  
7. Provide ability for the pan supplied with each drawer to lift straight out of standard width Drawer Warmers 20.75” x 12.75” x 6”.  
8. Unit shall have completely insulated individual cavities.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.