ITEM #: HEATED FOOD TRANSPORT CABINET MOBILE  
Quantity: One (1)  
Manufacturer: Carter Hoffmann  
Model No.: BB90  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 13.7A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide completely welded double wall cabinet construction with outer cabinet formed and welded to base.  
4. Provide type 300 series stainless steel; 20-gauge polished exterior and 24-gauge interior.  
5. Provide unit with 8” larger balloon casters, with four-wheel brakes.  
6. Provide wrap around bumper of non-marking gray vinyl bumper set in heavy-duty 3/16” thick extruded aluminum frame with reinforced corner cut outs.  
7. Provide one door with concealed stainless steel hinges with 5/16” pin.  
8. Provide flush mounted heavy-duty sliding latch with exclusive grip handle.  
9. Provide dial type with remote sensing bulb and sensing bulb protector, mounted to center mullion.  
10. Provide bottom mounted heater.  
11. Provide 90 covered plate capacity.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.