ITEM #: HEATED HOLDING CABINET  
Quantity: One (1)  
Manufacturer: Alto-Shaam  
Model No.: 750-TH-II  
Pertinent Data: Mobile  
Utilities Req’d: 120V/1PH; 14.2A (From Item #\_\_)

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide single compartment Halo Heat® Cook & Hold Oven constructed with a stainless steel exterior.  
3. Oven to include a stainless steel door with magnetic latch.  
4. Equip oven with two (2) stainless steel side racks with eleven (11) pan positions spaced on 1-3/8" (35mm) centers, three (3) stainless steel wire shelves, one (1) stainless steel drip pan with drain, and one (1) external drip tray.  
5. Provide one (1) set of 2-1/2" casters — 2 rigid, and 2 swivel with brake.  
6. Equip oven with one (1) simple control with On/Off power switch.  
7. Provide cook temperature knob, 200°F to 325°F (94°C to 160°C); hold temperature knob 60°F to 205°F (16°C to 96°C).  
8. Provide digital display, and up/down arrows to set cook and hold time.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.