ITEM #: HEATED PLATE DISPENSER  
Quantity: One (1)  
Manufacturer: Dinex  
Model No.: DDPEH21200W  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 7.5A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a two silo, heated plate dispenser.  
4. Unit shall have all welded stainless steel construction with #3 polished finish. Cabinet has 8-gauge top and 20-gauge side panels.  
5. Equip unit with self-leveling dispensers which are constructed of stainless steel and travel vertically in dispenser tube with nylon guides for smooth operation.  
6. Provide dispenser with flange mounted perimeter extension springs, which are detachable to provide adjustment without tools.  
7. Unit shall be equipped with a heating system which is thermostatically controlled, in a tamper protective location. Thermostat is field adjustable with a temperature range between 100 to 189 degrees. On/off switch and power indicator light are mounted on top flange of dispenser.  
8. Equip unit with four non-marking plastic corner bumpers.  
9. Provide four (4) 5” swivel casters, two (2) with brakes.  
10. Coordinate installation with Item #???.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.