ITEM #: HOT / COLD SHELF  
Quantity: One (1)  
Manufacturer: Hatco  
Model No.: HCSBF-48-S  
Pertinent Data: Self-Contained Refrigeration  
Utilities Req'd: 120V/1PH; 11.5A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation into Item #, Buffet Counter.  
4. Provide ability of shelves to change from hot to cold, and cold to hot in as little as 30 minutes.  
5. Provide unit with thermal breaks.  
6. Provide long, flexible copper refrigerant line, with ability to pull out condensing unit, results in easy service and installation.  
7. Provide hard coat aluminum shelf top mount.  
8. Provide electronic temperature control and condensing unit.  
9. Control box shall be mounted on stainless steel apron of Item #, Buffet Counter.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.