ITEM # : HOT CHOCOLATE DISPENSER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: FMD-3 Black (SET00.0197)  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 15.0A; 1/4” CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide adjustable legs and drip tray accommodate 20oz mugs easily.  
4. Equip with attractive high-impact resin door which is dent and scratch resistant.  
5. Provide electrical and plumbing components easily accessible through front and top.  
6. Provide high speed heavy-duty whipper for complete product mixing.  
7. Equip with improved automatic rinsing of whipper which reduces run-on after beverage is dis-pensed.  
8. Equip with large easy-to-fill translucent hoppers hold 4 lbs of product each, ensuring quick and timely refilling.  
9. Unit shall have lighted front graphics for merchandising are easy to exchange: cappuccino or soup.  
10. Provide variable speed motors allow control of product consistency in mixing chamber (.75 to 6.6 grams of powder per second).  
11. Coordinate installation onto Item #\_\_\_\_\_.  
12. Must meet all applicable governmental, and local laws, rules, regulations, and codes.