ITEM #: HOT TOP RANGE  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: IHR-2HT   
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 120,000BTU’s; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a 20mm rear LP Gas connection.  
4. Provide an oven with a high-performance stainless steel unique burner at 35,000 Btu/hour.  
5. Provide two heavy-duty, highly polished tops which provide even heat across entire surface.  
6. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
7. Provide “U” shaped burners that have 12 KW output.  
8. Provide porcelainized interior sides rear and deck on oven.  
9. Provide 1219mm flex, quick disconnect gas hose with restraining device and LP gas pressure regulator.  
10. Provide PosiSet.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.