ITEM # : HOT WATER DISPENSER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: H3X ELEMENT SST (45300.0006)  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 11.2A, 1/4" CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with heavy duty cord, coordinate with electrical contractor.  
3. Provide unit with digital thermostat which provides consistent and precise temperatures from 60° - 212°F.  
4. Provide unit with Push and Hold dispense -with one programmable Portion Control setting for a volume of up to 2 gallons.  
5. Equip unit with an LED display which provides simple temperature adjustment.  
6. Unit shall be equipped with Thinsulate7 tank insulation provides increased energy efficiency.  
7. Provide programmable "Energy Saver Mode" reduces operating costs during idle periods.  
8. Coordinate installation onto Item #\_\_\_\_\_.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.