ITEM #: ICE BIN  
Quantity: One (1)  
Manufacturer: Kloppenberg  
Model No.: SPS-3  
Pertinent Data: 2,000 Pounds Capacity  
Utilities Req’d: (2) 1” IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate opening in top of bin with Item #\_\_\_\_, Ice Machine, and Item #\_\_\_, Ice Machine.  
3. Provide guillotine style dispensing with three (3) guillotine ice shut-off.  
4. Provide all trims required for proper installation.  
5. Provide stainless steel construction.  
6. Provide three polycarts.  
7. Provide 1-1/2" foamed in-place polyurethane insulation.  
8. Provide adjustable flanged feet.  
9. Provide one (1) 48” UHMWP ice paddle.  
10. Provide stainless steel tubular base with cart drain center rear  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.