ITEM #: ICE CUTTING SAW  
Quantity: One (1)  
Manufacturer: Hobart  
Model No.: 6614  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 6.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a direct gear drive transmission.  
4. Unit shall have a tri-rail carriage.  
5. Provide an open frame stainless steel construction.  
6. Unit shall be equipped with a center crown pulley.  
7. Provide unit with removable double flanged pulleys.  
8. Provide a split rear table.  
9. Provide direction grain stainless steel.  
10. Unit shall be equipped with pivoted automatic tension.  
11. Equip unit with adjustable legs.  
12. Provide a movable carriage tray with stainless steel turned down edges, a stepped front edge, six stainless steel ball bearings, mounted on under-side of carriage, and a carriage lock.  
13. Equip unit with a rugged gauge plate with a stainless steel plate on aluminum cast frame, 6-3/4” x 16-3/4”, adjustment gives quick, positive regulation of cut thickness with precision, easily disengaged for adjustment.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.