ITEM #: ICE FLAKER  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: F0522W-1A  
Pertinent Data: 420 Pounds Capacity, Water Cooled  
Utilities Req’d: 220V/50/1PH, 15.0A each; 3/8" CW (from #\_\_\_), 1" IW, 1/2" Condenser Water In - 40 PSI @ 40-50 deg. F, 1/2" Condenser Water Out  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce flaked ice.  
6. Must meet all applicable governmental, and local laws, rules, regulations, and codes.