ITEM #: ICE FLAKER  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: F0822R-1  
Pertinent Data: 580 Pounds ARI Capacity, Air Cooled  
Utilities Req’d: 120V/1PH, 18.3A; 3/8" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice machine and Item #\_\_\_\_\_, Water Filtration System.  
 4. Install ice machine on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice machine shall produce flaked Ice.  
6. Provide unit with Vari-Smart Ultrasonic Ice Level Control.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin flawlessly.  
8. Coordinate installation and hook unit up to Item #\_\_\_\_\_,Remote Condenser.