ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: F-1002MWJ  
Pertinent Data: 833 Pounds ARI Capacity, Self-Contained Refrigeration   
Utilities Req’d: 120V/1PH, 13.7A; 1/2" CW, 3/4" IW, 1/2" Chilled Water Supply,

3/8" Chilled Water Return  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce Cublet Ice.  
6. Provide unit with H-GUARD Plus Antimicrobial Agent.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.