ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: F-801MAJ  
Pertinent Data: 566 lb/266 kG Capacity, Air Cooled  
Utilities Req'd: 208V/1PH, 11.0A; 1/2" CW, 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless-steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice machine shall produce nugget ice.  
6. Provide unit with an installation kit.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.