ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: FD-650MAJ-C  
Pertinent Data: 634 Pounds ARI Capacity, Self-Contained Refrigeration   
Utilities Req’d: 120V/1PH, 11.3A; 1/2" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and and Item #\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce Cublet Ice.  
6. Provide unit with H-GUARD Plus Antimicrobial Agent.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.