ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: FM-300AKE-HCN-SB  
Pertinent Data: 550 Pounds, Air-Cooled, Flake Ice  
Utilities Req’d: 120V/1PH, 3.9A; 3/4” CW, 3/4” IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have efficient ice making process due to Hoshizaki’s unique auger system.  
3. Unit will utilize all water brought into the machine; therefore, water consumption is equal to ice production.  
4. Provide an auger that is made of double hardened stainless steel. Combined with carbon bearings, they work optimally in a tough and wet environment. Benefits include: longer product life expectancy and reduced maintenance costs.  
5. Equip with micro computer controlled, controlling the ice making process to perform at its best under varying circumstances, without having to make physical adjustments.  
6. Unit shall have an easily cleanable air filter allows end users to carry out a routine cleaning schedule, extending product life expectancy and reducing the frequency and costs of maintenance callouts.  
7. Unit shall produce 55o Pounds nugget ice per 24 hours.  
8. Coordinate installation onto Item #\_\_\_\_, Ice Bin.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.