ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: IM-240XNE-HC-32  
Pertinent Data: 418 lb/190 kG Capacity, Air Cooled  
Utilities Req'd: 208V/1PH, 4.0A; 1/2" CW, 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless-steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice machine shall produce crescent cubes 1-1/4" x 1-1/4" x 1-1/4" (32mm x 32mm x 32mm).  
6. Provide unit with an installation kit.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_, Ice Bin flawlessly.  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.