ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: KM-1100MAJ  
Pertinent Data: 935 lb/424 kG Capacity, Air Cooled  
Utilities Req'd: 208V/1PH, 12.5A; 1/2" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless-steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice machine shall produce crescent cubes 1/2" x 1-1/8" x 1-1/2" (15mm x 33.7mm x 38.1mm).  
6. Provide unit with an installation kit.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_, Ice Bin flawlessly.  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.