ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: KMD-410MAJ  
Pertinent Data: 351 lb AHRI Capacity  
Utilities Req’d: 120V/1PH, 8.2A; 1/2" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless-steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_, Ice Bin, coordinate proper installation.  
5. Ice machine shall produce crescent cubes 1/2" x 1-1/8" x 1-1/2".  
6. Provide unit with an installation kit.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.