ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: C0630MW-32  
Pertinent Data: 600 Pounds Capacity, Water Cooled  
Utilities Req’d: 208V/1PH,9.8A; 3/8” CW, 3/4” IW; 3/8” Chilled Water Supply,   
 1/2” Chilled Water Return  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce medium cube ice 7/8” x 7/8” x 7/8”.  
6. Provide unit with KPAS which includes KVS VariSmart Ice Level Control, and KSBUN Smart Board Advance Control with Network.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.